                            INSTALLATION OVERVIEW

Follow these steps to install the Above Board Plus and Plus I/O.  Refer to
the Above Board manual for details about each step.

1  Add memory to the Above Board and insert the Above Board in the computer.

2  Make a back-up of the Intel diskette to use for installing the software.

3  Run the SETBOARD program to set up the board's hardware.

4  Run the computer's setup program (for 80286-based computers only) if you
   use the Above Board to add conventional or extended memory.

5  Run the TESTAB (confidence tests) program to pinpoint non-functioning or
   improperly installed RAM chips on the Above Board.

6  If you are using Above Boards other than Above Board Plus or Plus I/O to
   supply expanded memory, run the ALT.BAT file so the proper version of 
   EMM.SYS will be installed.

7  Run the INSTALL program to install the Above Board software that lets you
   use expanded memory, RAM disks, and a print buffer. 
